\pagebreak

Block name: I\_SenseAmp

Number of inputs: 2

Number of outputs: 1

Parameter list: I\_SenseAmp\_ota0\_ibias, I\_SenseAmp\_fgota0\_ibias, I\_SenseAmp\_fgota0\_pbias, I\_SenseAmp\_fgota0\_nibias, I\_SenseAmp\_cap0, I\_SenseAmp\_cap1

Block description: 
A Current Sense Amplifier block using an OTA, an FG OTA, and two capacitors. Ibias1 is I\_SenseAmp\_ota0\_ibias, which has a default value of 2$\mu$A. Ibias2 is I\_SenseAmp\_fgota0\_ibias, which has a default value of 2$\mu$A. The FGOTA's pbias is I\_SenseAmp\_fgota0\_pbias, which has a default value of 2$\mu$A. The FGOTA's nbias is I\_SenseAmp\_fgota0\_nbias, which has a default value of 2$\mu$A. It has two capacitor variables, which are I\_SenseAmp\_cap0 and I\_SenseAmp\_cap1.

\begin{figure}[H]  % jpg, png, or pdf
\includegraphics[width=300pt]{/home/ubuntu/rasp30/sci2blif/documentation/blocks_latex/figures/I_SenseAmp.pdf}
\end{figure}

