\pagebreak

Block name: adc\_ip

Number of inputs: 1

Number of outputs: 0

Parameter list: none

Block description: 
ADC (8bit 20MHz) is an 8-bit CMOS A/D converter (TAD3308A), which is a TSMC IP blcok. The cell receives analog input signal and decodes to digital output signals. Sampling rate is controlled by the clock input signal.

\begin{figure}[H]  % jpg, png, or pdf
\includegraphics[width=300pt]{/home/ubuntu/rasp30/sci2blif/documentation/blocks_latex/figures/adc_ip.pdf}
\end{figure}

