\pagebreak

Block name: fgota

Number of inputs: 2

Number of outputs: 1

Parameter list: Ibias, Vfg\_n, Vfg\_n, small\_cap

Block description: 
A nine transistor OTA block with input FG devices, which is one analog element blocks. Ibias controls the bais current. Vfg\_n and Vfg\_p define input FG pFET's floated node voltage, respectively.

\begin{figure}[H]  % jpg, png, or pdf
\includegraphics[width=300pt]{/home/ubuntu/rasp30/sci2blif/documentation/blocks_latex/figures/fgota.pdf}
\end{figure}

