\pagebreak

Block name: VolDivide1

Number of inputs: 1

Number of outputs: 1

Parameter list: VolDivide1\_ota0\_ibias, VolDivide1\_fgota0\_ibias, VolDivide1\_fgota0\_pbias, VolDivide1\_fgota0\_nbias

Block description: 
A Voltage divider block using an OTA and an FG OTA. Ibias1 is VolDivide1\_ota0\_ibias, which has a default value of 2$\mu$A. Ibias2 is VolDivide1\_fgota0\_ibias, which has a default value of 2$\mu$A. The FGOTA's pbias is VolDivide1\_fgota0\_pbias, which has a default value of 2$\mu$A. The FGOTA's nbias is VolDivide1\_fgota0\_nbias, which has a default value of 2$\mu$A. 

\begin{figure}[H]  % jpg, png, or pdf
\includegraphics[width=300pt]{/home/ubuntu/rasp30/sci2blif/documentation/blocks_latex/figures/VolDivide1.pdf}
\end{figure}

